Willian

**Configuração loja Santa Helena**

**Configuração SW-SH-01**

interface range fastEthernet 0/2 – 4

channel-protocol pagp

channel-group 1 mode desirable

Interface Port-channel 1

Switchport mode trunk

Interface fastEthernet 0/1

Switchport mode trunk

Vtp mode server

Vtp domain DOM

Vtp password dom

Vtp version 2

Vlan 10

Name CAIXA

Vlan 20

Name ESTOQUE

Vlan 30

Name ESCRITORIO

interface range fastEthernet 0/5 - 6

switchport mode access

switchport access vlan 10

**Configuração SW-SH-02**

interface range fastEthernet 0/2 – 4

channel-protocol pagp

channel-group 1 mode auto

Interface Port-channel 1

Switchport mode trunk

interface range fastEthernet 0/5 – 7

channel-protocol pagp

channel-group 2 mode desirable

Interface Port-channel 2

Switchport mode trunk

Vtp mode client

Vtp password dom

Vtp version 2

interface range fastEthernet 0/8 - 9

switchport mode access

switchport access vlan 20

**Configuração SW-SH-03**

interface range fastEthernet 0/5 – 7

channel-protocol pagp

channel-group 2 mode auto

Switchport mode trunk

Vtp mode client

Vtp password dom

Vtp version 2

interface range fastEthernet 0/1 - 2

switchport mode access

switchport access vlan 30

**Configuração RT-SH**

Interface GigabitEthernet 0/0

No shut

interface GigabitEthernet 0/0.10

encapsulation dot1Q 10

ip address 196.168.1.30 255.255.255.224

interface GigabitEthernet 0/0.20

encapsulation dot1Q 20

ip address 196.168.1.62 255.255.255.224

interface GigabitEthernet 0/0.30

encapsulation dot1Q 30

ip address 196.168.1.94 255.255.255.224